//Roll No. : 32410

//Problem statement: Program to obtain

//square wave output by interfacing DAC0808 to 8051

#include<reg51.h>

void msDelay(unsigned int);

void main(void){

P1=0x00;

while(1){

P1=~P1;

msDelay(50);

}

}

void msDelay(unsigned int t){

unsigned int i,j;

for(i=0;i<t;i++)

for(j=0;j<1275;j++){}

}