//Roll No. :32410

//Problem Statement: Program to obtain

//sinewave output by interfacing DAC0808 to 8051

#include<reg51.h>

void main()

{

unsigned int sinvalue[12]={128,192,238,255,238,192,128,64,17,0,17,64};

unsigned int i;

while(1)

{

for(i=0;i<12;i++)

{

P1=sinvalue[i];

}

}

}